|  |  |
| --- | --- |
|  **Model Picture** |  |
| **Q2000** | **Q1500** |
| Rated AC Output | 2200W | 1500W |
| Rated Capacity | 2016Wh | 1440Wh  |
| Standard Capacity | 48V/42Ah or 3.2V/630000mAh | 48V/30Ah or 3.2V/450000mAh |
| Bettery Type | LiFePO4 |
| UPS | YES |
| Charging Temperature Range | 0℃~40℃ |
| **ChargeWay** | AC Input | 1200W |
| DC Input | NO |
| Car Charge | 12V/10A(120W)  |
| Solar Charge (MPPT) | 800W |
| **USB Output** | USB-Type-C | PD 100W\*2 |
| USB-A | QC3.0\*4(72W max) |
| DC port Output | 12V/5A\*2(120W) |
| Cigarret Lighter Output | 12V/10A(120W)  |
| LED Light | SOS,Flshlingt(8W) |
| **AC Output** | Output waveform | Pure Sine Wave  |
| Output voltage  | 110V/220V  |
| Output frequency  | 50/60Hz |
| AC continuous output | 2200W | 1500W |
| Peak AC output | 4400W | 3000W |
| Maximum device power that can be worked | 4400W | 3000W |
| Discharging Temperature Range |  -10~40℃  |
| Authentication  | UL,FCC,CE,ROSH,PSE,UN38.3,SAA,UKCA |
| Product Size | 410\*290\*290mm |
| Weight | about22kg | about18kg |
| Warrantly | 18 months |
| Accessories |  portable power supply 1\*User Manual color box packaging 1\*MC4 charging cable 1\*vehicle charging cable1\*AC cable  |  portable power supply 1\*User Manual color box packaging 1\*MC4 charging cable 1\*vehicle charging cable1\*AC cable  |