|  |  |  |  |
| --- | --- | --- | --- |
| **Model Picture** | |  | |
| **Q2000** | **Q1500** |
| Rated AC Output | | 2200W | 1500W |
| Rated Capacity | | 2016Wh | 1440Wh |
| Standard Capacity | | 48V/42Ah or  3.2V/630000mAh | 48V/30Ah or  3.2V/450000mAh |
| Bettery Type | | LiFePO4 | |
| UPS | | YES | |
| Charging Temperature Range | | 0℃~40℃ | |
| **Charge Way** | AC Input | 1200W | |
| DC Input | NO | |
| Car Charge | 12V/10A(120W) | |
| Solar Charge (MPPT) | 800W | |
| **USB Output** | USB-Type-C | PD 100W\*2 | |
| USB-A | QC3.0\*4(72W max) | |
| DC port Output | | 12V/5A\*2(120W) | |
| Cigarret Lighter Output | | 12V/10A(120W) | |
| LED Light | | SOS,Flshlingt(8W) | |
| **AC Output** | Output waveform | Pure Sine Wave | |
| Output voltage | 110V/220V | |
| Output frequency | 50/60Hz | |
| AC continuous output | 2200W | 1500W |
| Peak AC output | 4400W | 3000W |
| Maximum device power that can be worked | 4400W | 3000W |
| Discharging Temperature Range | | -10~40℃ | |
| Authentication | | UL,FCC,CE,ROSH,PSE,UN38.3,SAA,UKCA | |
| Product Size | | 410\*290\*290mm | |
| Weight | | about22kg | about18kg |
| Warrantly | | 18 months | |
| Accessories | | portable power supply 1\*User Manual color box packaging 1\*MC4 charging cable 1\*vehicle charging cable 1\*AC cable | portable power supply 1\*User Manual color box packaging 1\*MC4 charging cable 1\*vehicle charging cable 1\*AC cable |